,Width##LENGTH##INCHES,Voltage Range##OTHER##,Voltage Option N##ELECTRICAL_POTENTIAL##VOLTS,Voltage Option F##ELECTRICAL_POTENTIAL##VOLTS,Service Clearance##OTHER##,Power Factor##OTHER##,Phase##OTHER##,Number of Poles##OTHER##,Low Voltage##ELECTRICAL_POTENTIAL##VOLTS,Voltage Option H##ELECTRICAL_POTENTIAL##VOLTS,Frequency##ELECTRICAL_FREQUENCY##HERTZ,Depth##LENGTH##INCHES,Height with Electrical Connections##LENGTH##INCHES,Height##OTHER##,Header Location 4##LENGTH##INCHES,Header Location 3##LENGTH##INCHES,Header Location 2##LENGTH##INCHES,Header Location 1##LENGTH##INCHES,Default Elevation[-1154647]##LENGTH##INCHES,Current##ELECTRICAL_CURRENT##AMPERES
HVAC_Modular_Chiller_ClimaCool_PW_50-80_Ton_Cabinet,30.000000000000,208-230 V,575.000000000000,460.000000000000,1,1,1,1,24.000000000000,208.000000000000,60.000000000000,60.000000000000,61.200000000000,73.54,61.200000000000,45.850000000000,25.750000000000,10.390000000000,0.000000000000,0.000000000000
