,Width##LENGTH##INCHES,Voltage Range##OTHER##,Voltage Option N##ELECTRICAL_POTENTIAL##VOLTS,Voltage Option F##ELECTRICAL_POTENTIAL##VOLTS,Power Factor##OTHER##,Phase##OTHER##,Number of Poles##OTHER##,Low Voltage##ELECTRICAL_POTENTIAL##VOLTS,Length##LENGTH##INCHES,Voltage Option H##ELECTRICAL_POTENTIAL##VOLTS,Height with Electrical Connections##LENGTH##INCHES,Height##LENGTH##INCHES,Header Location 4##LENGTH##INCHES,Header Location 3##LENGTH##INCHES,Header Location 2##LENGTH##INCHES,Header Location 1##LENGTH##INCHES,Frequency##ELECTRICAL_FREQUENCY##HERTZ,Default Elevation[-1154647]##LENGTH##INCHES,Service Access Zones (default)##OTHER##,Current##ELECTRICAL_CURRENT##AMPERES
Not a Type - Load Type Catalog!,24.000000000000,208-230 V,575.000000000000,460.000000000000,1,3,3,24.000000000000,55.000000000000,208.000000000000,72.510000000000,70.000000000000,61.160000000000,45.800000000000,25.710000000000,10.350000000000,60.000000000000,0.000000000000,1,0.000000000000
